WhisperKOOL® Exterior Housing for Split Systems

* Galvanized steel base and steel cabinet embossed — 20 GA, hinged access for easier servicing
* Easily assembled in the shop or on the job
* Rain Trough under hinge to catch moisture that might seep through the hinge
* WhisperKOOL® provides fasteners
* 20” W x 20” H x 27”D

Our exterior condenser housing protects the condenser portion of the split system from the elements when installed outdoors. Exterior Condenser Housing is used with the Platinum Mini Split, Ductless Platinum Split, and Ducted Platinum Split cooling units.

WhisperKOOL® Extreme Ducting Plenum

* Ducting plenum for the evaporator and condenser of the Extreme ti
* Duct the evaporator or condenser side of the unit to ­fit your installation needs
* Small is compatible with Extreme 3500ti and 5000ti
* Large is compatible with Extreme 8000ti
* WhisperKOOL® provides fasteners

Sizes available for the 3500ti, 5000ti, and 8000ti. This plenum allows either side of the unit to be ducted. Duct the cold air through a vent into the cellar, duct the hot exhaust air out of the home. This plenum allows for total installation flexibility.

WhisperKOOL® Extreme Exterior Grille

* Protects your Extreme ti through-the-wall unit from the elements of weather
* Small is compatible with 3500ti and 5000ti
* Large is compatible with 8000ti
* WhisperKOOL® provides ½” pan-head screws

The Exterior Grille protects the exhaust side of the system from the weather elements when installed through an exterior wall.

WhisperKOOL® SC Exterior Grille

* Protects your SC through-the-wall unit from the elements of weather
* Small is compatible with 2000i, 3000i, and 4000i
* Large is compatible with 6000i and 8000i
* WhisperKOOL® provides ½” pan-head screws

The Exterior Grille protects the exhaust side of the system from the weather elements when installed through an exterior wall.

WhisperKOOL® SC Ducting Kit

* Small is compatible with 2000i, 3000i, and 4000i
* Large is compatible with 6000i and 8000i
* ONLY the exhaust side of the SC can be ducted
* WhisperKOOL® does not provide ducting

This kit allows the warm exhaust air to be ducted to another area. Ideal if the room adjacent to your cellar is not ideal for warm air to be exhausted into. The kit includes the Thermostat Controller, which will turn on and push warm exhaust air away from the

ducting (not included). The in-line fan can be set to automatically turn on at varying temperatures in order to conserve the most electricity.

Small Duct works on the SC 2000i/3000i/4000i and XLT 1600/3000/4200. Kit includes:

* Duct Plenum
* Transition with integrated heat sensor
* 8″ In-line fan
* 8″ Adjustable Elbow

Large Duct works on the SC 6000i/8000i and XLT 6000/8000. Kit includes:

* Duct Plenum
* Transition with integrated heat sensor
* 8″ In-line fan with transitions to 8″
* 8″ Adjustable Elbow